|  |
| --- |
| 1. **AXIOM Core − a platform for managing distributed CCTV systems**   **REPLIKANT Sp. z o.o.**  Axiom Core is a platform for managing distributed CCTV systems. Its main feature is support for the protection of facilities thanks to integration with SSWIN and the sales department using Business Intelligence. It provides a high level of security through detailed supervision over access to the system and encryption of communication. Dedicated software and hardware increase the flexibility and efficiency of the system, which translates into real financial benefits. |
| 1. **Correspondence depositor**   **BT ELECTRONICS Sp. z o.o.**  SAIK POSTAL are electronic lockers of various sizes for receiving and transmitting external and internal correspondence. Dedicated software informs the right people about new content in real time via e-mail and / or text messages. The large touch screen enables easy and clear collection, for example, of a new letter, and the system architecture will prevent unauthorised access to the content. The steel structure ensures safe storage of all contents. |
| 1. **New sensor cable controller dLISTcontroller using SEC15 cable with SECcon quick connectors**   **Listec GmbH / CREATIO Arkadiusz Waligóra**  The modern dLISTcontroller increases your safety by significantly reducing operating and service costs and the negative impact on the environment: - flexibility of the system thanks to its modular structure and SECcon quick couplers - high resistance to external and environmental factors - extensive communication possibilities thanks to a large number of inputs and outputs, as well as the use of the MODBUS protocol - low power consumption: 210 mA - environmentally friendly - effectively protects green energy and critical infrastructure against fire. |
| 1. **Wisenet TNO-7180R − IP camera for recognising car plates with Global shutter**   **HANWHA TECHWIN EUROPE LTD**  Wisenet TNO-7180R is a camera designed to monitor and inform about the current situation on motorways and expressways. Resolution of up to 3 MPix, 60 fps, 18x magnification, integration with adaptive IR illuminator and support of Global Shutter technology provides the ability to read licence plates from 50 metres in complete darkness. The analytics that recognises the direction of movement and the tracking of the object enables the camera to work in various scenarios. |
| 1. **ZUP-230V-BM − Air intake gates power supply in gravity smoke exhaust systems**   **MERAWEX Sp. z o. o.**  ZUP-230V-BM is a series of power adapters with power range from 400 to 1500W, which provide guaranteed voltage of 230V AC and optionally 24Vdc. They are intended to supply controllers and drives of gates which, during a fire, are used to support the building’s smoke exhaust, acting as air intake gates. The power adapter can work with any Fire Alarm Control Panel. ZUP-230V-BM are manufactured by MIRAWEX and are provided with the Certificate of Constancy of Performance and the Certificate of Release to Service issued by Polish Scientific and Research Centre for Fire Protection − National Research Institute. |